;File of English for program Color 6.2

[GENERAL]
language=English


[STARTING_PAGE_NEWS]
Title_1=THE REGISTRATION:
SubTitle_11=- Are Changed registration keys;
SubTitle_12=
SubTitle_13=
SubTitle_14=
SubTitle_15=

Title_2=THE HOLDERS of the FUZES:
SubTitle_21=- a new types (75 names);
SubTitle_22=
SubTitle_23=
SubTitle_24=
SubTitle_25=

Title_3=THE REFERENCE DATA:
SubTitle_31=- A Color coding of importances TFC;
SubTitle_32=
SubTitle_33=
SubTitle_34=
SubTitle_35=

Title_4=LANGUAGE SUPPORT:
SubTitle_41=- A New points;
SubTitle_42=
SubTitle_43=
SubTitle_44=
SubTitle_45=

Title_5=CASE:
SubTitle_51=- A new types;
SubTitle_52=- Added analogues;
SubTitle_53=
SubTitle_54=
SubTitle_55=

[DLG_ABOUTPROGRAM]
logo=About program Color
comment=(information on versions, date of the issue, author...)
STATIC1=Program "COLOR" Version 6.2
STATIC2=On themes
STATIC3="Determination element REE on color
STATIC4=and code marking + reference book"
STATIC5=December 24 2006
STATIC7=On program worked:
STATIC8=Programmer -
STATIC9=Guest book
STATIC10=Site of the program Color http://ColorAndCode.narod.ru
STATIC11=Forum

[MENU_FILE]
file=File
print=Print...
printsetup=Page Setup...
exit=Exit

[MENU_VIEW]
view=View
toolbars=Toolbar
statusbar=Status Bar

[MENU_ELEMENTS]
elements=Elements
newcalculation=New calculation
marks=Marks
standards=Standards
modechipcomponent=Mode chip component
modecapacitor=The Mode capacitor
resistors=Resistors
capacitors=Capacitors
transistors=Transistors
diodes=Diodes
stabilitronyandstabistors=Stabilitrony and stabistors
varikapy=Varikapy
inductances=Inductances
chipcomponents=Chip components

[MENU_ELEMENTS_MARKS]
1_mark=1 Mark
2_marks=2 Marks
3_marks=3 Marks
3_marksin=3 Marks (inwardly branded)
4_marks=4 Marks
5_marks=5 Marks
6_marks=6 Marks
codemarking=Code marking
nonstandclrmark=Non-standard color marking
nonstandcodemark=Non-standard code marking
horizontalmarking=Horizontal marking
verticalmarking=Vertical marking
mixedmarking=Mixed marking
series81x=Series 81x
series3x=Series 3x

[MENU_ELEMENTS_STANDARDS]
gost_62iec=GOST/62 IEC
philips=PHILIPS
cgw=CORNING GLASS WORK
panasonic=PANASONIC
codeGOST_62_115_2IEC=Code GOST/62 and 115-2 IEC
bourns=BOURNS
smd=SMD capacitors
ru=Domestic
proel=PRO ELECTRON
sod_123=In case SOD-123

[MENU_ELEMENTS_MODECHIPCOMPONENT]
chipresistors=Chip resistors
chipcapacitors=Chip capacitors
chipdiodes=Chip diodes

[MENU_ELEMENTS_MODECAPACITOR]
color_marking=Color marking
code_marking=Code marking

[MENU_SERVICE]
service=Service
calculator=Calculator
referencebook=Reference book
modereferencebook=Mode of the reference book
informationbase=Information on base
language=Language

[MENU_SERVICE_MODEREFERENCEBOOK]
Table=Table
body=Case

[MENU_REFERENCE_DATA]
referencedata=Reference data
rows=Rows of importances
tr=Tiporazmery
pp_alem=Indication semiconductor instrument
color_code=Color marking

[MENU_REFERENCE_DATA_TR]
chip_r=Chip resistors import
chip_c=Chip capacitors

[MENU_REFERENCE_PP_ALEM]
pp_alem_guest=GUEST 10862-64 (four elements)

[MENU_REFERENCE_DATA_KONTUR_IMP_PRIEM]
kontur_imp_priem=Contour spools import radio
color_cod_tke=Coding of importances TFC

[MENU_REFERENCE]
reference=Reference
help=Help
aboutprogram=About program
registration=Registration

[MENU_WHEREBUY]
wherebuy=WHERE BUY ?
whatbuyprogram=What buy program Color
informationforadvertisers=Information for advertisers

[STARTING_PAGE]
startingpage=STARTING PAGE
newpossibilities=NEW POSSIBILITIES
detailreadreference=In detail read reference section 'NEW POSSIBILITIES'
determination=DETERMINATION
elementreaon=ELEMENT REE ON
colorandcode=COLOR AND CODE
marking=MARKING
referencebook=REFERENCE BOOK
registrationrequired=Registration is Required

[MESSAGEBOX]
attention=Attention
registration=Registration
invalidnumber=The invalid number are Incorporated!
faithfullnumber=The faithfull number are Incorporated.
givenfunctionrequiredregistration=For use given function is required registration.

[DLG_BUYCOLOR]
dlgbuycolor=What buy program Color
paymentwebmoney=Payment through Web Money
paymentbank=Payment through bank

[DLG_BUYCOLOR_WM]
STATIC1=For aquisition of the program necessary to pay 3.0 WMZ / 90.0 WMR with patronage of the deal
STATIC2=on purse:
STATIC4=After undertaking the payment you will send us their own data:
STATIC5=- Your name
STATIC9=- Name and version of the program
STATIC10=on address
STATIC11=and we shall send You: personal and registration number.
attestatinfo=Is it Here found certificate our WM identifier 147957655434
STATIC12=You buy one version, but the following new versions get gratis.
STATIC13=or
STATIC14=Payment through service Web Merchant Interface - WMZ
STATIC15=Payment through service Web Merchant Interface - WMR

[DLG_BUYCOLOR_BANK]
STATIC1=If you do not use Webmoney, that will be able to pay program by bank payment
STATIC2=in rouble through payment system PayBox.ru
STATIC3=The Amount to payment will form 250 roubles.
STATIC4=Page with form for filling data

[DLG_REGISTRATION]
logo=Registration
comment=(the choice of the type to registrations...)
STATIC1=Pay version - Shareware
STATIC2=Personal number
STATIC3=Registration number
STATIC4=- Polnofunkcionalinaya program
STATIC5=Free version - Freeware
STATIC6=Not available following elements of management
STATIC7=With author on e-mail possible
produceregistration=PRODUCE REGISTRATION
transistors=- Transistors
nonstandclrmark=Non-standard color marking;
nonstandcodemark=Non-standard code marking;
mixedmarking=Mixed marking;
resistors=- Resistors
codemarking=Code marking;
capacitors=- Capacitors
fivecolourmarkings=five colour markings;
codemarkings=code marking;
chip=Chip components.
determinationinductances=The Determination of the inductances.
elementmanagementReferencebook=The Element of management 'Reference book.
conclusionelement=The Conclusion of the features element.
determinationdiode=The Determination diode.

[DLG_INFORMATIONONBASE]
logo=Information on element base
comment=(the name of the base, amount element, file...)
elementbase=Element base
amountdetails=Amount of the details
namefile=Name of the file
conclusionanalogue=Conclusion analogue
transistors=Transistors
diodes=Diodes
stabilitronyandstabistors=Stabilitrony and stabistors
varikapy=Varikapy
stabilizers=Stabilizers
body=Case
holdersfuzes=Holders of the fuzes
optopary=Optopary
wholeelement=Whole element

[DLG_PARALPOSLEDREZ]
calculator=Parallel and consequent join resistor
paralleljoin=Parallel join
consequentjoin=Consequent join
withprovisionpossibledeflection=With provision for possible deflection in %
calculation=The calculation

[DLG_CALCULATOR]
logo=Calculator
comment=Calculations of the different technical direction
calc_1=Parallel and consequent join resistor

[DLG_REFERENCEBOOK]
logo=Reference book
STATIC1=Searching for
STATIC2=The Element base
STATIC3=The Subgroup

[DLG_REFERENCEBOOK_BASE]
transistors=The Transistors
diodes=The Diodes
stabilitronystabistors=Stabilitrony and stabistors
varikapy=Varikapy
stabilizers=The Stabilizers
body=The case
holdersfuzes=The Holders of the fuzes
optopary=Optopary

[DLG_REFERENCEBOOK_SUBGROUP]
allelements=All elements
diode=Diode
transistor=Transistor
bipolar_npn_usual=Bipolar n-p-n usual
bipolar_pnp_usual=Bipolar p-n-p usual
bipolar_npn_component=Bipolar n-p-n component
bipolar_pnp_component=Bipolar p-n-p component
transistor_assemblies_npn_bipolar=The Transistor assemblies n-p-n bipolar
transistor_assemblies_pnp_bipolar=The Transistor assemblies p-n-p bipolar
transistor_assemblies_npn_and_pnp_bipolar=The Transistor assemblies n-p-n and p-n-p bipolar
one_connecting_n_base=One connecting n-base
field_pn_transition_channel_n_type=Field p-n transition channel n-type
field_pn_transition_channel_p_type=Field p-n transition channel p-type
usual=Usual
hung_radiating=It Is Hung radiating
IK_range=IK-range
stabilitrony_general_purpose=Stabilitrony general-purpose
stabilitrony_precizion=Stabilitrony прецизионные
stabilitrony_pulsed=Stabilitrony pulsed
stabilitrony_two_anode=Stabilitrony two anode
stabistors=The Stabistors
linear_positive_voltage=The Linear positive voltage
linear_negative_voltage=The Linear negative voltage
controlled=Controlled
pulsed_voltages=The Pulsed voltages
montage_on_charge=The Montage on charge
on_wire=On wire
car_fuzes=For car fuzes

[MESSAGES_REFERENCEBOOK]
GUIDETO=THE GUIDE TO
TRANSISTOR=TRANSISTOR
DIODE=DIODE
STABILITRONYSTABISTOR=STABILITRONY AND STABISTOR
VARIKAPY=VARIKAPY
STABILIZER=STABILIZER
BODY=CASE
HOLDERFUZES=HOLDER OF THE FUZES
OPTOPARY=OPTOPARY

[MESSAGES_STATUSBAR]
SB_FILE_PRINT=Print feature of the selected element
SB_FILE_PRINT_SETUP=Adjust parameters of the seal or printer
SB_APP_EXIT=Terminate work with program Color

SB_SHOW_TOOL=Show or hide toolbar
SB_VIEW_STATUS_BAR=Show or hide status bar

SB_NEW_CALC=Begin calculation of the new element (N)
SB_REZ=Choose calculation a resistor
SB_KOND=Choose calculation a capacitor
SB_TRANZ=Choose the calculation a transistor
SB_DIOD=Choose the calculation a diode
SB_STAB=Choose the calculation stabilitrony and stabistor
SB_VAR=Choose the calculation an varikapy
SB_INDUKT=Choose the calculation of the inductances
SB_CHIP=Choose the calculation a chip component

SB_KALKULATOR=Calculations of the different technical direction (K)
SB_SPRAVOCHNIK=Call to reference information on element base
SB_INFO_BASE=The Conclusion to information (the amount element...) on element base
SB_ROWS=Rows of importances of the resistances and capacities
SB_TR_CHIP_R=Tiporazmery chip resistor for surrface montage import
SB_TR_CHIP_C=Tiporazmery laminated ceramic beskorpucnyh chip capacitor
SB_PP_ALEM_GOST=Indication semiconductor instrument
SB_COLOR_CODE_KONTUR_IMP_PRIEM=Color marking contour spool import radio
SB_COLOR_COD_TKE=Color coding of importances TFC

SB_HELP_FINDER=Description of the program (F1)
SB_APP_ABOUT=Information on product: versions, date...
SB_REGISTRATION=Produce registration of the program

SB_BUY_COLOR=Information on buying the program Color
SB_INFO_REAKLAMA=Information on how to place information on Your company in program

SB_M_1=On element is inflicted one mark (1)
SB_M_2=On element are inflicted two marks (2)
SB_M_3=On element are inflicted three marks (3)
SB_M_3_IN=On element are inflicted three marks inwardly branded marking
SB_M_4=On element are inflicted four marks (4)
SB_M_5=On element is inflicted five marks (5)
SB_M_6=On element is inflicted six marks (6)
SB_M_X=On element are inflicted code marks (X)
SB_NS_COLOR=Non-standard color marks are inflicted On element
SB_NS_CODE=Non-standard code marks are inflicted On element
SB_GORIZ=Horizontal code marking is inflicted On element
SB_VERTIK=Vertical code marking is inflicted On element
SB_SMESHAN=Mixed marking is inflicted On element
SB_81X=Transistors to serieses 81x
SB_3X=Transistors to serieses 3x

SB_R_GOST=Standard resistor in accordance with GOST17598-72 and requirements to Publications 62 IEC
SB_R_PHILIPS=Standard resistor PHILIPS
SB_R_CGW=Standard resistor CORNING GLASS WORK
SB_R_PANASONIC=Standard resistor PANASONIC
SB_R_X=Code marking in accordance with GUEST 11076-69 and requirements Publication 62 and 115-2 IEC
SB_R_BOURNS=Standard resistor BOURNS
SB_SMD=Code marking electrolytic capacitor for surrface montage - SMD
SB_SOD_123=In case SOD-123
SB_RU=Domestic marking
SB_PROEL=Marking on standard PRO ELECTRON

SB_CHIP_R=Choose calculation a chip resistor
SB_CHIP_C=Choose calculation a chip capacitor
SB_CHIP_D=Choose calculation a chip diode

SB_COLOR_MODE_CAPACITOR=Mode of the color marking capacitor
SB_CODE_MODE_CAPACITOR=Mode of the code marking capacitor

SB_MODE_SPRAV_TABL=Image of the features in the manner of tables
SB_MODE_SPRAV_KORPUS=Image gabarit sizes of the case

SB_LANGUAGE=Choice of the language of the program


SB_IDS_IDLEMESSAGE=Press F1 for reception help

[MESSAGES_TOOLBAR]
TB_NEW_CALC=New calculation
TB_REZ=Resistors
TB_KOND=Capacitors
TB_TRANZ=Transistors
TB_DIOD=Diodes
TB_STAB=Stabilitrony and stabistors
TB_VAR=Varikapy
TB_INDUKT=Inductances
TB_CHIP=Chip components
TB_R_GOST=GOST/62 IEC
TB_R_PHILIPS=PHILIPS
TB_R_CGW=CORNING GLASS WORK
TB_R_PANASONIC=PANASONIC
TB_R_X=Code GOST/62 and 115-2 IEC
TB_R_BOURNS=BOURNS
TB_SMD=SMD capacitors
TB_SOD_123=SOD-123
TB_SPRAVOCHNIK=Reference book
TB_MODE_SPRAV_TABL=Table
TB_MODE_SPRAV_KORPUS=Case
TB_FILE_PRINT=Print
TB_M_1=One mark
TB_M_2=Two marks
TB_M_3=Three marks
TB_M_3_IN=Three marks - inwardly branded
TB_M_4=Four marks
TB_M_5=Five marks
TB_M_6=Six marks
TB_M_X=Code marks
TB_NS_COLOR=Non-standard color marks
TB_NS_CODE=Non-standard code marks
TB_GORIZ=Horizontal marking
TB_VERT=Vertical marking
TB_SMESHAN=Mixed marking
TB_81X=Series 81x
TB_3X=Series 3x
TB_CHIP_R=Chip resistors
TB_CHIP_C=Chip capacitors
TB_CHIP_D=Chip diodes
TB_COLOR_MODE_CAPACITOR=Color marking
TB_CODE_MODE_CAPACITOR=Code marking
TB_RU=Domestic
TB_PROEL=PRO ELECTRON

[DLG_ROWS]
logo=Rows of importances of the resistances and capacities

[DLG_SELECT_LANGUAGE]
logo=Language...
comment=(choice of the language of the program)
cancel=Cancel

[DLG_TR_CHIP_RC]
logo_1=Tiporazmery chip resistor for surrface montage import
logo_2=Tiporazmery laminated ceramic unpackaged chip capacitor
tr=Tiporazmer
mass=Mass (gram)

[TITLE]
typebody=type of the case
CAPACITOR=CAPACITOR
SMD=SMD
DETERMINATION_CHIP=DETERMINATION CHIP
RESISTOR_ON=RESISTOR ON
DETERMINATION_TYPE_TRANSISTOR=THE DETERMINATION of the TYPE of the TRANSISTOR
DETERMINATION_NOMINAL_RESISTOR=DETERMINATION of the NOMINAL VALUE of the RESISTOR ON
DETERMINATION_NOMINAL_CAPACITOR=DETERMINATION of the NOMINAL VALUE of the CAPACITOR ON
DETERMINATION_TYPE_DIODE=DETERMINATION of the TYPE of the DIODE ON
DETERMINATION_TYPE_DIODE_SOD_123=DETERMINATION of the TYPE of the DIODE In BODY SOD-123
DETERMINATION_TYPE_STABILITRON=DETERMINATION of the TYPE STABILITRONS And STABISTOR ON
DETERMINATION_TYPE_VARIKAPA=DETERMINATION of the TYPE VARIKAPA ON
DETERMINATION_NOMINAL_INDUCTANCES=DETERMINATION of the NOMINAL VALUE of the INDUCTANCES ON
POINT_COLOUR_MARKING=POINT COLOUR MARKING
COLOUR_MARKING=COLOUR MARKING
CODE_MARKING=CODE MARKING
MARKING_1_O=1-e
MARKING_2_X=2-o
ON_MARKING_2_X=ON 2-o
MARKING_3_X=3-e
ON_MARKING_3_X=ON 3-e
MARKING_3_h_inwardly_branded=3-h (inwardly branded)
MARKING_4_X=4-r
MARKING_5_I=5-e
MARKING_6_I=6-s
SERIESES_3x=THE SERIESES 3x
SERIESES_81x=THE SERIESES 81x
HORIZONTAL_MARKING=ON HORIZONTAL MARKING
VERTICAL_MARKING=ON VERTICAL MARKING
MIXED_MARKING=ON MIXED MARKING
NON_STANDARD_CODE_MARKING=ON NON-STANDARD CODE MARKING
NON_STANDARD_COLOR_MARKING=ON NON-STANDARD COLOR MARKING
ON_CODE_MARKING=ON CODE MARKING
ON_2x_POINT_COLOR_MARKING=ON 2-x POINT COLOR MARKING
ON_4x_POINT_COLOR_MARKING=ON 4-x POINT COLOR MARKING
STANDART_PROEL=STANDARD PRO ELECTRON

[MESSAGES_PROGRAM]
MP_DETERMINATION=DETERMINATION :
MP_RESULT=RESULT :
MP_IMPORTANCE_NOT_FOUND=IMPORTANCE is NOT FOUND
MP_BOURNS_M3=For resistor from row E-24, the tolerance 1 and 5%, type size 0603, 0805 and 1206.
MP_BOURNS_M3_IN=For resistor from row E-96, the tolerance 1%, type by size 0603.
MP_BOURNS_M4=For resistor from row E96, the tolerance 1%, type size 0805 and 1206.
MP_PANASONIC_R_VID_0_1=Ring of the wanted colour marks
MP_PANASONIC_R_VID_0_2=high-quality film resistor
MP_PANASONIC_R_VID_0_3=type ERDAS3 for sound technology

[DLG_PP_ALEM_GOST]
logo=Indication semiconductor instrument on GUEST 10862-64 (four elements)
TITLE_1=Element and purpose
TITLE_2=Conditional indication
TITLE_ALEM_1=THE FIRST ELEMENT - a SOURCE MATERIAL:
ALEM_1_G=- Germanium
ALEM_1_K=- Silicon
ALEM_1_A=- Arsenide галия and his(its) join
TITLE_ALEM_2=SECOND ELEMENT - a SUBCLASS INSTRUMENT :
ALEM_2_1=- Sverhvysokochastotnye diodes
ALEM_2_2=- Varikapy
ALEM_2_3=- Vypryamitelinye, universal, pulsed diodes
ALEM_2_4=- Tunelinye diodes
ALEM_2_5=- Uncontrolled laminated switching instruments
ALEM_2_6=- Stabilitrony
ALEM_2_7=- Transistors
ALEM_2_8=- Operated laminated switching instruments
ALEM_2_9=- Fotopribory
ALEM_2_10=- Vypryamitelinye poles and blocks
TITLE_ALEM_3=THE THIRD ELEMENT - a PURPOSE INSTRUMENT :
ALEM_3_1=+ Diodes low and radio frequency
ALEM_3_1_1=- выпрямительные
ALEM_3_1_2=- universal
ALEM_3_1_3=- pulsed
ALEM_3_2=+ Varikapy
ALEM_3_3=+ SVCH-DIODES
ALEM_3_3_1=-mixing
ALEM_3_3_2=-video detectors
ALEM_3_3_3=-модуляторные
ALEM_3_3_4=-parametric
ALEM_3_3_5=-switching
ALEM_3_3_6=-умножительные
ALEM_4_1=+ Photodiodes
ALEM_5_1=+ Phototransistors
ALEM_6_1=+ Operated laminated switching instruments (thyristors)
ALEM_6_1_1=-small power
ALEM_6_1_2=-average power
ALEM_6_1_3=-big power
ALEM_7_1=+ Uncontrolled laminated switching instruments (динисторы)
ALEM_7_1_1=-small power
ALEM_7_1_2=-average power
ALEM_7_1_3=-big power
ALEM_8_1=+ Tunelinye diodes
ALEM_8_1_1=- усилительные
ALEM_8_1_2=- генераторные
ALEM_8_1_3=- switching
ALEM_9_1=+ Stabilitrony with voltage of the stabilizations, V
ALEM_9_1_1=* small power (P < 0,3 Vt) :
ALEM_9_1_2=* average power (P = 0,3...5 Vt) :
ALEM_9_1_3=* big power (P > 5 Vt) :
ALEM_10_1=+ Vypryamitelinye poles
ALEM_10_1_1=- small power
ALEM_10_1_2=- average power
ALEM_11_1=+ Vypryamitelinye blocks
ALEM_11_1_1=- small power
ALEM_11_1_2=- average power
ALEM_11_1_3=- big power
ALEM_12_1=+ Transistors
ALEM_12_1_1=* small power
ALEM_12_1_1_1=- low frequency
ALEM_12_1_1_2=- average frequency
ALEM_12_1_1_3=- high and over radio frequency
ALEM_12_1_2=* average power
ALEM_12_1_2_1=-l ow frequency
ALEM_12_1_2_2=- average frequency
ALEM_12_1_2_3=- high and over radio frequency
ALEM_12_1_3=* big power
ALEM_12_1_3_1=-l ow frequency
ALEM_12_1_3_2=- average frequency
ALEM_12_1_3_3=- high and over radio frequency
TITLE_ALEM_4=THE FOURTH ELEMENT - a letter, marking taxonomic group of the instrument (the variety of the type).
Example=The Example. KT315A - a transistor on base silicon, small power, radio frequency.

[DLG_COLOR_CODE_INDUK_IMP_PRIEM]
logo=Color marking contour spool import radio
TITLE_1=Colour of the marking
TITLE_2=Purpose contour spool
TITLE_3=Number conclusion windings
TITLE_4=Number whorl
TITLE_5=Capacity of the internal capacitor, pf
TITLE_6=Picture

KONTUR_1_color=Yellow
KONTUR_1_purpose=Filter IF-АМ - 455...460 кГц 
KONTUR_1_numberconclusion=1-2-3 / 4-6
KONTUR_1_numberwhorl=100+50
KONTUR_1_capacity=190

KONTUR_2_color=White
KONTUR_2_purpose=Detector IF-АМ - 455...460 кГц 
KONTUR_2_numberconclusion=1-2-3
KONTUR_2_numberwhorl=50+50
KONTUR_2_capacity=410

KONTUR_3_color=Orange
KONTUR_3_purpose=Filter IF-FМ - 10,7МГц [*]
KONTUR_3_numberconclusion=1-3 / 4-6
KONTUR_3_numberwhorl=12 / 2 
KONTUR_3_capacity=75

KONTUR_4_color=Lilac
KONTUR_4_purpose=Filter IF-FМ - 10,7 МГц 
KONTUR_4_numberconclusion=1-3 / 4-6
KONTUR_4_numberwhorl=11 / 2
KONTUR_4_capacity=90

KONTUR_5_color=Rose
KONTUR_5_purpose=Discriminator IF-FМ - 10,7 МГц [**]
KONTUR_5_numberconclusion=1-3
KONTUR_5_numberwhorl=7
KONTUR_5_capacity=190

KONTUR_6_color=Green or blue 
KONTUR_6_purpose=Discriminator IF-FМ - 10,7 МГц [**]
KONTUR_6_numberconclusion=1-3
KONTUR_6_numberwhorl=11

KONTUR_7_color=Red
KONTUR_7_purpose=Sidebar гетеродина АМ AW-LW 
KONTUR_7_numberconclusion=1-3 / 4 - 6, 2 - 3 
KONTUR_7_numberwhorl=80...100 [***] / 8...12 
KONTUR_7_capacity=-

KONTUR_COMENT_1=[*] Can be used instead of blue and green. In this case spool relationship 4-6 are not connected to charge.
KONTUR_COMENT_2=[**] They Are Used with different microcircuit.
KONTUR_COMENT_3=[***] The Number whorl depends on capacities CVC. The Correlation of the number whorl windings of the contour spool and spools relationship are chose within 10:1-8:1.

[DLG_COLOR_CODE_TKE]
logo=Color coding of importances TFC

TITLE_1=Colour of the case
TITLE_2=Colour point on case
TITLE_3=Group TFC
TITLE_4=Importance TFC, 10^-6/*C, in interval of the temperature 20...85 *C

blue1=blue
gray=gray
blue2=blue
black=black
brown=brown
red=red
orange=orange
yellow=yellow
green=green
yellow_or_gray=yellow or gray
